FBQ1: The most common items found on a motherboard are \_\_\_.

Answer: Sockets

FBQ2: A \_\_\_\_ is described as a device that communicates with the computer and interprets the data on the storage media associated with the drive devices.

Answer: Drive

FBQ3: The Central Processing Unit is commonly referred to as a \_\_\_

Answer: Processor

FBQ4: Joysticks are input devices specially designed for some computer \_\_\_.

Answer: Games

FBQ5: Most scanners have the ability to convert \_\_ images into actual texts.

Answer: Text

FBQ6: Within the context of Software Application Skills, the acronym OCR stands for the \_\_ Character Recognition.

Answer: Optical

FBQ7: Generally, the \_\_\_ is an input device that records voice data to the computer.

Answer: Microphone

FBQ8: The process of using the computer to participate in discussion with a group of people in a distant place is referred to as \_\_\_\_ conferencing.

Answer: Video

FBQ9: \_\_\_\_ devices are used to convey the results of computer processing.

Answer: Output

FBQ10: The monitor is one of the most common \_\_\_\_ devices.

Answer: Display

FBQ11: The printer is a common \_\_ device.

Answer: Output

FBQ12: The keyboard is a standard \_\_\_ unit.

Answer: Input

FBQ13: Just like the television set, the monitor uses the same \_\_\_ Ray Tube .

Answer: Cathode

FBQ14: The acronym LCD stands for the \_\_ Crystal Display.

Answer: Liquid

FBQ15: One of the earliest forms of the printer is the \_\_\_\_ Matrix Printers.

Answer: Dot

FBQ16: Printers are employed for obtaining \_\_\_ copies of output of computer processing.

Answer: Hard

FBQ17: \_\_\_ Matrix printers belong to the group of printers classified as Impact Printers

Answer: Dot

FBQ18: The term \_\_\_ refers to the number of dots per inch.

Answer: Resolution

FBQ19: An \_\_ jet printer output produces blots when hands are rubbed on the paper after printing.

Answer: Ink

FBQ20: \_\_\_ jet and inkjet printers are classified as non-impact printers

Answer: Laser

FBQ21: \_\_\_ that come with your multimedia pack are classified as sound devices

Answer: Speakers

FBQ22: Laser \_\_\_\_ colour printers are usually very expensive

Answer: Jet

FBQ23: Normally, \_\_\_ are required to play audio files.

Answer: Speakers

FBQ24: Television channel signals can be received on ones computer by installing a suitable \_\_\_\_ device.

Answer: Communication

FBQ25: Storage devices are also referred to as auxiliary \_\_ devices.

Answer: Memory

FBQ26: The most common keyboard has \_\_\_\_\_ number of keys.

Answer: 104

FBQ27: Ordinarily, LCD panels are flat in shape and thereby decrease the desk space when used with \_\_\_ computers.

Answer: Desktop

FBQ28: When the Caps Lock key is pressed, an indicator light at the top right corner of the \_\_\_ appears.

Answer: Keyboard

FBQ29: Within the context of software application skills, Alphanumeric keys are also referred to as the \_\_\_\_ keys.

Answer: Editing

FBQ30: Today, the layouts of most electronic keyboards closely follow that of the \_\_\_ keyboard.

Answer: QWERTY

FBQ31: Ordinarily, the Tab key is used to indent \_\_\_ and is frequently used in paragraphing.

Answer: Texts

FBQ32: The \_\_ key is also known as the Return key.

Answer: Enter

FBQ33: Editing keys consist of the character keys, \_\_\_ keys on the second row and some keys associated with text inputs.

Answer: Numeric

FBQ34: The term for the order of characters on the back row of keys, from left to right, on a manual typewriter is the \_\_.

Answer: Qwerty

FBQ35: The process of using the mouse to select items is described as \_\_\_\_ .

Answer: Highlighting

MCQ1: Within the context of software applications, the \_\_\_ key is used to indent texts and is often employed in paragraphing.

Answer: Tab

MCQ2: Arithmetic and \_\_\_ operations are the basic CPU operations

Answer: Logical

MCQ3: The input device that records voice data to the computer is the \_\_\_

Answer: Microphone

MCQ4: Once the following combination of keys: Ctrl + Alt + Del are pressed, the computer system \_\_\_\_ .

Answer: Reboots

MCQ5: Within the context of software application skills, the acronym ENIAC represents the \_\_\_\_.

Answer: Electronic Numerical Integrator And Calculator

MCQ6: The world’s first electrical computers were referred to as \_\_\_\_.

Answer: MARK I

MCQ7: Ada Byron is acknowledged as the first Computer \_\_\_\_\_\_.

Answer: Programmer

MCQ8: Babbage's \_\_\_\_ engine could store intermediate results in a memory unit

Answer: Analytical

MCQ9: \_\_\_\_ is the input device specially designed for computer games.

Answer: Joystick

MCQ10: Babbage devised an engine for computing logarithm \_\_\_ and printing the results.

Answer: Tables

MCQ11: The \_\_\_\_ Automatic Computer was the first commercial electronic computer.

Answer: Universal

MCQ12: The \_\_\_ generation computers made use of Large Scale Integrated circuits and Very Large Scale Integrated circuits.

Answer: Fourth

MCQ13: \_\_\_\_ computers are very large and so are specially housed in big buildings.

Answer: Mainframe

MCQ14: The \_\_\_\_ generation computers are those developed to mimic human intelligence.

Answer: Fifth

MCQ15: Ordinarily, the CPU is located on the \_\_\_\_\_\_.

Answer: Motherboard

MCQ16: Babbage's engine could store \_\_\_\_\_\_ results in a memory unit.

Answer: Intermediate

MCQ17: The \_\_\_\_\_\_ is the first computer to perform arithmetic and logical operations using a stored-program.

Answer: EDSAC

MCQ18: The historical development of the computer can be divided into \_\_\_\_\_\_ phases.

Answer: Four

MCQ19: The Hard Disk Drive is equally referred to as the \_\_ Disk Drive.

Answer: Fixed

MCQ20: The \_\_\_\_ is commonly regarded as the brain of the computer system.

Answer: Central Processing Unit

MCQ21: Originally, Babbage machines were\_\_\_ in designs

Answer: Mechanical

MCQ22: The acronym EDSAC represents the \_\_\_\_\_\_

Answer: Electronic Delay Storage Automatic Computer

MCQ23: The first computer program was developed for Babbage's \_\_\_ Engine

Answer: Analytical

MCQ24: The \_\_\_\_ generation computers used Integrated Circuits

Answer: 3rd

MCQ25: Within the context of mainframes, they \_\_ are referred to as the medium-sized computers.

Answer: Minicomputers

MCQ26: The \_\_\_\_ interconnects directly or indirectly all the other computer devices.

Answer: Motherboard

MCQ27: The major component of Windows that has tools for managing computer devices is the control \_\_\_..

Answer: Panel

MCQ28: The \_\_ unit mainly oversees the data movement between the Arithmetic Logic Unit and the Main Memory.

Answer: Control

MCQ29: Ordinarily, 1 Gigabyte is equivalent to \_\_ bytes.

Answer: I, 073, 741,824

MCQ30: The memory size of a \_\_\_ density diskette is twice that of a 720KB memory.

Answer: High

MCQ31: The Date/Time component allows one to update the date and time \_\_\_ on a computer.

Answer: Settings

MCQ32: The \_\_\_ panel component is used to configure the desktop wallpaper

Answer: Control

MCQ33: Usually, \_\_\_ units are used to transfer commands and data into the computer system.

Answer: Input

MCQ34: The term BIT is derived from two words namely: \_\_\_ and digital.

Answer: Binary

MCQ35: The control unit of the CPU operates in the Fetch- \_\_\_\_ cycle.

Answer: Execute